**FEATURES:**  
grease gun coupler(Hydraulic grease nipples,H1 straight)  
4 jaws turned.  
connect machine with injection packer  
steel, galvanized  
Pressure: 4500psi-10000 psi

Connection1 For H1-nipples  
Connection2 G1/8 female  
Design 4jaws  
Wrench size (mm) 13  
Material yellow, zinc  
Diameter 15  
Length 36  
Weight (kg) 0.03