**FEATURES:**
grease gun coupler(Hydraulic grease nipples,H1 straight)
4 jaws turned.
connect machine with injection packer
steel, galvanized
Pressure: 4500psi-10000 psi

Connection1 For H1-nipples
Connection2 G1/8 female
Design 4jaws
Wrench size (mm) 13
Material yellow, zinc
Diameter 15
Length 36
Weight (kg) 0.03